**Before the**

**Federal Communications Commission**

**Washington, D.C. 20554**

|  |  |  |
| --- | --- | --- |
| In the Matter of  Revision of Part 15 of the Commission’s Rules to  Permit Unlicensed National Information  Infrastructure (U-NII) Devices in the 5 GHz Band | **)**  **)**  **)**  **)**  **)**  **)**  **)**  **)** | ET Docket No. 13-49 |

**ERRATUM**

**Released: September 30, 2014**

By the Chief, Office of Engineering and Technology:

On April 1, 2014, the Commission released a *First Report and Order* (*First R&O*), FCC 14-30, in the above captioned proceeding. This Erratum amends Appendix C of the *First R&O* as indicated below:

In paragraph (iii) of section 15.407(a)(1), following the first sentence, add a new sentence to read as “In addition, the maximum power spectral density shall not exceed 17 dBm in any 1 megahertz band.”

FEDERAL COMMUNICATIONS COMMISSION

Julius P. Knapp

Chief, Office of Engineering and Technology